BackEnd - Python Module

end

Respond to client with HTTP JSON response

Generate JSON from sensor data

Read Current Value and Find apparent power from current and voltage (230v)

Initialize DHT11 and Current ADC (CT) Driver

http request from mirror?

Listen for client connection

Read Humidity and Temperature value. Evaluate DewPoint